           CPU0       CPU1       
  8:          0          0  xen-pirq-ioapic-edge  rtc0
  9:          0          0  xen-pirq-ioapic-level  acpi
 20:         33          0  xen-pirq-ioapic-level  ehci_hcd:usb1
 23:      57716          0  xen-pirq-ioapic-level  ehci_hcd:usb2
 40:      49152          0  xen-percpu-virq      timer0
 41:         16          0  xen-percpu-ipi       spinlock0
 42:      87551          0  xen-percpu-ipi       resched0
 43:          0          0  xen-percpu-ipi       callfunc0
 44:          0          0  xen-percpu-virq      debug0
 45:       4952          0  xen-percpu-ipi       callfuncsingle0
 46:       4153          0  xen-percpu-ipi       irqwork0
 47:          0      50137  xen-percpu-virq      timer1
 48:          0         29  xen-percpu-ipi       spinlock1
 49:          0     134100  xen-percpu-ipi       resched1
 50:          0          0  xen-percpu-ipi       callfunc1
 51:          0          0  xen-percpu-virq      debug1
 52:          0       3913  xen-percpu-ipi       callfuncsingle1
 53:          0      13277  xen-percpu-ipi       irqwork1
 54:          0          0   xen-dyn-event     xenbus
 55:          0          0   xen-dyn-virq      xen-pcpu
 56:          0          0  xen-pirq-msi       PCIe PME
 57:          0          0  xen-pirq-msi       PCIe PME
 58:          0          0  xen-pirq-msi       PCIe PME
 59:          0          0   xen-dyn-virq      mce
 61:     110439          0  xen-pirq-msi       ahci
 62:       2234          0  xen-pirq-msi       eth0
 63:          4          0  xen-pirq-msi       eth1
NMI:          0          0   Non-maskable interrupts
LOC:          0          0   Local timer interrupts
SPU:          0          0   Spurious interrupts
PMI:          0          0   Performance monitoring interrupts
IWI:       4153      13277   IRQ work interrupts
RTR:          0          0   APIC ICR read retries
RES:      87551     134100   Rescheduling interrupts
CAL:       4952       3913   Function call interrupts
TLB:          0          0   TLB shootdowns
TRM:          0          0   Thermal event interrupts
THR:          0          0   Threshold APIC interrupts
MCE:          0          0   Machine check exceptions
MCP:          2          2   Machine check polls
ERR:          0
MIS:          0
