 __  __            _  _    __    _ 
 \ \/ /___ _ __   | || |  / /_  / |
  \  // _ \ '_ \  | || |_| '_ \ | |
  /  \  __/ | | | |__   _| (_) || |
 /_/\_\___|_| |_|    |_|(_)___(_)_|
                                   
(XEN) [    0.000000] Xen version 4.6.1-xs125300-d (root@) (gcc (GCC) 4.8.5 20150623 (Red Hat 4.8.5-4)) debug=y Mon May  9 10:01:14 UTC 2016
(XEN) [    0.000000] Latest ChangeSet: c0cfb7220a84, pq e3524863b7ea
(XEN) [    0.000000] Bootloader: SYSLINUX 4.07 2013-07-25
(XEN) [    0.000000] Command line: dom0_max_vcpus=1-2 dom0_mem=1024M,max:1024M com1=115200,8n1 console=com1,vga
(XEN) [    0.000000] Video information:
(XEN) [    0.000000]  VGA is text mode 80x25, font 8x16
(XEN) [    0.000000]  VBE/DDC methods: V2; EDID transfer time: 1 seconds
(XEN) [    0.000000] Disc information:
(XEN) [    0.000000]  Found 4 MBR signatures
(XEN) [    0.000000]  Found 5 EDD information structures
(XEN) [    0.000000] Xen-e820 RAM map:
(XEN) [    0.000000]  0000000000000000 - 000000000009dc00 (usable)
(XEN) [    0.000000]  000000000009dc00 - 00000000000a0000 (reserved)
(XEN) [    0.000000]  00000000000e0000 - 0000000000100000 (reserved)
(XEN) [    0.000000]  0000000000100000 - 00000000bdfb0000 (usable)
(XEN) [    0.000000]  00000000bdfb0000 - 00000000bf3b0000 (reserved)
(XEN) [    0.000000]  00000000bf3b0000 - 00000000bf5ce000 (usable)
(XEN) [    0.000000]  00000000bf5ce000 - 00000000bf5d0000 (reserved)
(XEN) [    0.000000]  00000000bf5d0000 - 00000000bf5eb000 (usable)
(XEN) [    0.000000]  00000000bf5eb000 - 00000000bf5ef000 (reserved)
(XEN) [    0.000000]  00000000bf5ef000 - 00000000bf5f0000 (usable)
(XEN) [    0.000000]  00000000bf5f0000 - 00000000bf601000 (reserved)
(XEN) [    0.000000]  00000000bf601000 - 00000000bf63f000 (usable)
(XEN) [    0.000000]  00000000bf63f000 - 00000000bf6bf000 (reserved)
(XEN) [    0.000000]  00000000bf6bf000 - 00000000bf7bf000 (ACPI NVS)
(XEN) [    0.000000]  00000000bf7bf000 - 00000000bf7f0000 (ACPI data)
(XEN) [    0.000000]  00000000bf7f0000 - 00000000bf800000 (usable)
(XEN) [    0.000000]  00000000bf800000 - 00000000c0000000 (reserved)
(XEN) [    0.000000]  00000000e0000000 - 00000000f0000000 (reserved)
(XEN) [    0.000000]  00000000feb00000 - 00000000feb04000 (reserved)
(XEN) [    0.000000]  00000000fec00000 - 00000000fec01000 (reserved)
(XEN) [    0.000000]  00000000fed10000 - 00000000fed1a000 (reserved)
(XEN) [    0.000000]  00000000fed1c000 - 00000000fed20000 (reserved)
(XEN) [    0.000000]  00000000fee00000 - 00000000fee01000 (reserved)
(XEN) [    0.000000]  00000000ffc00000 - 0000000100000000 (reserved)
(XEN) [    0.000000]  0000000100000000 - 0000000140000000 (usable)
(XEN) [    0.000000] ACPI: RSDP 000FE020, 0024 (r2 DELL  )
(XEN) [    0.000000] ACPI: XSDT BF7EF170, 00A4 (r1 DELL   PE_SC3          1 DELL    40000)
(XEN) [    0.000000] ACPI: FACP BF7EB000, 00F4 (r4 DELL   PE_SC3          1 DELL    40000)
(XEN) [    0.000000] ACPI: DSDT BF7E1000, 68FE (r1 DELL   PE_SC3          0 DELL    40000)
(XEN) [    0.000000] ACPI: FACS BF7B8000, 0040
(XEN) [    0.000000] ACPI: SPMI BF7EE000, 0040 (r5 DELL   PE_SC3          1 DELL    40000)
(XEN) [    0.000000] ACPI: DMAR BF7ED000, 0078 (r1 DELL   PE_SC3          1 DELL    40000)
(XEN) [    0.000000] ACPI: ASF! BF7EC000, 00A5 (r32 DELL   PE_SC3          1 DELL    40000)
(XEN) [    0.000000] ACPI: HPET BF7EA000, 0038 (r1 DELL   PE_SC3          1 DELL    40000)
(XEN) [    0.000000] ACPI: APIC BF7E9000, 0092 (r2 DELL   PE_SC3          1 DELL    40000)
(XEN) [    0.000000] ACPI: MCFG BF7E8000, 003C (r1 DELL   PE_SC3          1 DELL    40000)
(XEN) [    0.000000] ACPI: BOOT BF7DE000, 0028 (r1 DELL   PE_SC3          1 DELL    40000)
(XEN) [    0.000000] ACPI: SSDT BF7DD000, 02F6 (r1 DELL   PE_SC3       1000 DELL    40000)
(XEN) [    0.000000] ACPI: ASPT BF7D9000, 0034 (r7 DELL   PE_SC3          1 DELL    40000)
(XEN) [    0.000000] ACPI: SSDT BF7D8000, 0A92 (r1 DELL   PE_SC3       3000 DELL    40000)
(XEN) [    0.000000] ACPI: SPCR BF7DA000, 0050 (r1 DELL   PE_SC3          1 DELL    40000)
(XEN) [    0.000000] ACPI: HEST BF7D7000, 00A8 (r1 DELL   PE_SC3          0 DELL    40000)
(XEN) [    0.000000] ACPI: ERST BF7D6000, 0230 (r1 DELL   PE_SC3          0 DELL    40000)
(XEN) [    0.000000] ACPI: BERT BF7D5000, 0030 (r1 DELL   PE_SC3          0 DELL    40000)
(XEN) [    0.000000] ACPI: EINJ BF7D4000, 0130 (r1 DELL   PE_SC3          0 DELL    40000)
(XEN) [    0.000000] System RAM: 4065MB (4163412kB)
(XEN) [    0.000000] No NUMA configuration found
(XEN) [    0.000000] Faking a node at 0000000000000000-0000000140000000
(XEN) [    0.000000] Domain heap initialised
(XEN) [    0.000000] found SMP MP-table at 000fe1b0
(XEN) [    0.000000] DMI 2.7 present.
(XEN) [    0.000000] Using APIC driver default
(XEN) [    0.000000] ACPI: PM-Timer IO Port: 0x408
(XEN) [    0.000000] ACPI: SLEEP INFO: pm1x_cnt[1:404,1:0], pm1x_evt[1:400,1:0]
(XEN) [    0.000000] ACPI:             wakeup_vec[bf7b800c], vec_size[20]
(XEN) [    0.000000] ACPI: Local APIC address 0xfee00000
(XEN) [    0.000000] ACPI: LAPIC (acpi_id[0x01] lapic_id[0x00] enabled)
(XEN) [    0.000000] ACPI: LAPIC (acpi_id[0x02] lapic_id[0x02] enabled)
(XEN) [    0.000000] ACPI: LAPIC (acpi_id[0x03] lapic_id[0x04] enabled)
(XEN) [    0.000000] ACPI: LAPIC (acpi_id[0x04] lapic_id[0x06] enabled)
(XEN) [    0.000000] ACPI: LAPIC (acpi_id[0x05] lapic_id[0x00] disabled)
(XEN) [    0.000000] ACPI: LAPIC (acpi_id[0x06] lapic_id[0x00] disabled)
(XEN) [    0.000000] ACPI: LAPIC (acpi_id[0x07] lapic_id[0x00] disabled)
(XEN) [    0.000000] ACPI: LAPIC (acpi_id[0x08] lapic_id[0x00] disabled)
(XEN) [    0.000000] ACPI: LAPIC_NMI (acpi_id[0xff] high edge lint[0x1])
(XEN) [    0.000000] ACPI: IOAPIC (id[0x00] address[0xfec00000] gsi_base[0])
(XEN) [    0.000000] IOAPIC[0]: apic_id 0, version 32, address 0xfec00000, GSI 0-23
(XEN) [    0.000000] ACPI: INT_SRC_OVR (bus 0 bus_irq 0 global_irq 2 dfl dfl)
(XEN) [    0.000000] ACPI: INT_SRC_OVR (bus 0 bus_irq 9 global_irq 9 high level)
(XEN) [    0.000000] ACPI: IRQ0 used by override.
(XEN) [    0.000000] ACPI: IRQ2 used by override.
(XEN) [    0.000000] ACPI: IRQ9 used by override.
(XEN) [    0.000000] Enabling APIC mode:  Flat.  Using 1 I/O APICs
(XEN) [    0.000000] ACPI: HPET id: 0x8086a201 base: 0xfed00000
(XEN) [    0.000000] [VT-D]  RMRR address range 0..fff not in reserved memory; need "iommu_inclusive_mapping=1"?
(XEN) [    0.000000] Xen ERST support is initialized.
(XEN) [    0.000000] HEST: Table parsing has been initialized
(XEN) [    0.000000] Using ACPI (MADT) for SMP configuration information
(XEN) [    0.000000] SMP: Allowing 8 CPUs (4 hotplug CPUs)
(XEN) [    0.000000] NR_CPUS:512 nr_cpumask_bits:64
(XEN) [    0.000000] IRQ limits: 24 GSI, 760 MSI/MSI-X
(XEN) [    0.000000] Switched to APIC driver x2apic_cluster.
(XEN) [    0.000000] xstate_init: using cntxt_size: 0x340 and states: 0x7
(XEN) [    0.000000] mce_intel.c:735: MCA Capability: BCAST 1 SER 0 CMCI 1 firstbank 0 extended MCE MSR 0
(XEN) [    0.000000] Thermal monitoring handled by SMI
(XEN) [    0.000000] Intel machine check reporting enabled
(XEN) [    0.000000] Using scheduler: SMP Credit Scheduler (credit)
(XEN) [    1.973536] Detected 3093.072 MHz processor.
(XEN) [    1.981570] Initing memory sharing.
(XEN) [    1.986830] alt table ffff82d08031c4e8 -> ffff82d08031d904
(XEN) [    1.994084] PCI: MCFG configuration 0: base e0000000 segment 0000 buses 00 - ff
(XEN) [    2.004499] PCI: MCFG area at e0000000 reserved in E820
(XEN) [    2.011494] PCI: Using MCFG for segment 0000 bus 00-ff
(XEN) [    2.018808] Intel VT-d iommu 0 supported page sizes: 4kB.
(XEN) [    2.026027] Intel VT-d Snoop Control enabled.
(XEN) [    2.032137] Intel VT-d Dom0 DMA Passthrough not enabled.
(XEN) [    2.039199] Intel VT-d Queued Invalidation enabled.
(XEN) [    2.045941] Intel VT-d Interrupt Remapping enabled.
(XEN) [    2.052502] Intel VT-d Shared EPT tables not enabled.
(XEN) [    2.066566] I/O virtualisation enabled
(XEN) [    2.072077]  - Dom0 mode: Relaxed
(XEN) [    2.077181] Interrupt remapping enabled
(XEN) [    2.082790] nr_sockets: 3
(XEN) [    2.087175] Enabled directed EOI with ioapic_ack_old on!
(XEN) [    2.094524] ENABLING IO-APIC IRQs
(XEN) [    2.099600]  -> Using old ACK method
(XEN) [    2.105398] ..TIMER: vector=0xF0 apic1=0 pin1=2 apic2=-1 pin2=-1
(XEN) [    2.313531] TSC deadline timer enabled
(XEN) [    2.493578] Platform timer is 14.318MHz HPET
(XEN) [    2.499217] Allocated console ring of 64 KiB.
(XEN) [    2.500627] mwait-idle: MWAIT substates: 0x1120
(XEN) [    2.502024] mwait-idle: v0.4.1 model 0x2a
(XEN) [    2.503426] mwait-idle: lapic_timer_reliable_states 0xffffffff
(XEN) [    2.505013] VMX: Supported advanced features:
(XEN) [    2.506403]  - APIC MMIO access virtualisation
(XEN) [    2.507790]  - APIC TPR shadow
(XEN) [    2.509060]  - Extended Page Tables (EPT)
(XEN) [    2.510473]  - Virtual-Processor Identifiers (VPID)
(XEN) [    2.511885]  - Virtual NMI
(XEN) [    2.513271]  - MSR direct-access bitmap
(XEN) [    2.514830]  - Unrestricted Guest
(XEN) [    2.516244] HVM: ASIDs enabled.
(XEN) [    2.517644] HVM: VMX enabled
(XEN) [    2.519032] HVM: Hardware Assisted Paging (HAP) detected
(XEN) [    2.520430] HVM: HAP page sizes: 4kB, 2MB
(XEN) [    2.522222] Brought up 4 CPUs
(XEN) [    2.546075] ACPI sleep modes: S3
(XEN) [    2.547463] VPMU: disabled
(XEN) [    2.548843] mcheck_poll: Machine check polling timer started.
(XEN) [    2.550246] Dom0 has maximum 408 PIRQs
(XEN) [    2.551633] csched_dom_init: setting dom 0 as the privileged domain
(XEN) [    2.553048] NX (Execute Disable) protection active
(XEN) [    2.554568] *** LOADING DOMAIN 0 ***
(XEN) [    2.704434] elf_parse_binary: phdr: paddr=0x1000000 memsz=0x883000
(XEN) [    2.705868] elf_parse_binary: phdr: paddr=0x1a00000 memsz=0xc00f0
(XEN) [    2.707280] elf_parse_binary: phdr: paddr=0x1ac1000 memsz=0x13900
(XEN) [    2.708623] elf_parse_binary: phdr: paddr=0x1ad5000 memsz=0x676000
(XEN) [    2.709997] elf_parse_binary: memory: 0x1000000 -> 0x214b000
(XEN) [    2.711414] elf_xen_parse_note: GUEST_OS = "linux"
(XEN) [    2.712804] elf_xen_parse_note: GUEST_VERSION = "2.6"
(XEN) [    2.714293] elf_xen_parse_note: XEN_VERSION = "xen-3.0"
(XEN) [    2.715741] elf_xen_parse_note: VIRT_BASE = 0xffffffff80000000
(XEN) [    2.717170] elf_xen_parse_note: ENTRY = 0xffffffff81ad51f0
(XEN) [    2.718588] elf_xen_parse_note: HYPERCALL_PAGE = 0xffffffff81001000
(XEN) [    2.720013] elf_xen_parse_note: FEATURES = "!writable_page_tables|pae_pgdir_above_4gb"
(XEN) [    2.722717] elf_xen_parse_note: PAE_MODE = "yes"
(XEN) [    2.724154] elf_xen_parse_note: LOADER = "generic"
(XEN) [    2.725607] elf_xen_parse_note: unknown xen elf note (0xd)
(XEN) [    2.727032] elf_xen_parse_note: SUSPEND_CANCEL = 0x1
(XEN) [    2.728437] elf_xen_parse_note: HV_START_LOW = 0xffff800000000000
(XEN) [    2.729864] elf_xen_parse_note: PADDR_OFFSET = 0x0
(XEN) [    2.731287] elf_xen_addr_calc_check: addresses:
(XEN) [    2.732693]     virt_base        = 0xffffffff80000000
(XEN) [    2.734188]     elf_paddr_offset = 0x0
(XEN) [    2.735600]     virt_offset      = 0xffffffff80000000
(XEN) [    2.736950]     virt_kstart      = 0xffffffff81000000
(XEN) [    2.738274]     virt_kend        = 0xffffffff8214b000
(XEN) [    2.739701]     virt_entry       = 0xffffffff81ad51f0
(XEN) [    2.741113]     p2m_base         = 0xffffffffffffffff
(XEN) [    2.742527]  Xen  kernel: 64-bit, lsb, compat32
(XEN) [    2.743979]  Dom0 kernel: 64-bit, PAE, lsb, paddr 0x1000000 -> 0x214b000
(XEN) [    2.747734] PHYSICAL MEMORY ARRANGEMENT:
(XEN) [    2.749088]  Dom0 alloc.:   0000000130000000->0000000134000000 (223026 pages to be allocated)
(XEN) [    2.751788]  Init. ramdisk: 000000013a732000->000000013ffffeb4
(XEN) [    2.753169] VIRTUAL MEMORY ARRANGEMENT:
(XEN) [    2.754642]  Loaded kernel: ffffffff81000000->ffffffff8214b000
(XEN) [    2.756031]  Init. ramdisk: ffffffff8214b000->ffffffff87a18eb4
(XEN) [    2.757392]  Phys-Mach map: ffffffff87a19000->ffffffff87c19000
(XEN) [    2.758763]  Start info:    ffffffff87c19000->ffffffff87c194b4
(XEN) [    2.760143]  Page tables:   ffffffff87c1a000->ffffffff87c5d000
(XEN) [    2.761513]  Boot stack:    ffffffff87c5d000->ffffffff87c5e000
(XEN) [    2.762890]  TOTAL:         ffffffff80000000->ffffffff88000000
(XEN) [    2.764409]  ENTRY ADDRESS: ffffffff81ad51f0
(XEN) [    2.768331] Dom0 has maximum 2 VCPUs
(XEN) [    2.769731] elf_load_binary: phdr 0 at 0xffffffff81000000 -> 0xffffffff81883000
(XEN) [    2.773936] elf_load_binary: phdr 1 at 0xffffffff81a00000 -> 0xffffffff81ac00f0
(XEN) [    2.776937] elf_load_binary: phdr 2 at 0xffffffff81ac1000 -> 0xffffffff81ad4900
(XEN) [    2.779644] elf_load_binary: phdr 3 at 0xffffffff81ad5000 -> 0xffffffff81bf2000
(XEN) [    3.312068] Masked UR signaling on 0000:00:00.0
(XEN) [    3.316356] Scrubbing Free RAM on 1 nodes using 4 CPUs
(XEN) [    3.342981] ..........done.
(XEN) [    3.519569] Initial low memory virq threshold set at 0x4000 pages.
(XEN) [    3.520979] Std. Loglevel: All
(XEN) [    3.522307] Guest Loglevel: All
(XEN) [    3.523626] Xen is relinquishing VGA console.
(XEN) [    3.525770] *** Serial input -> DOM0 (type 'CTRL-a' three times to switch input to Xen)
(XEN) [    3.526090] Freed 360kB init memory.
(XEN) [    3.593002] traps.c:2880:d0v0 Domain attempted WRMSR 00000000c0000081 from 0xe023e00800000000 to 0x0023001000000000.
(XEN) [    3.593007] traps.c:2880:d0v0 Domain attempted WRMSR 00000000c0000082 from 0xffff82d0bffff000 to 0xffffffff81551140.
(XEN) [    3.593010] traps.c:2880:d0v0 Domain attempted WRMSR 00000000c0000083 from 0xffff82d0bffff020 to 0xffffffff81549340.
(XEN) [    3.593013] traps.c:2880:d0v0 Domain attempted WRMSR 0000000000000174 from 0x000000000000e008 to 0x0000000000000010.
(XEN) [    3.593017] traps.c:2880:d0v0 Domain attempted WRMSR 0000000000000175 from 0xffff8300bdd27fc0 to 0x0000000000000000.
(XEN) [    3.593020] traps.c:2880:d0v0 Domain attempted WRMSR 0000000000000176 from 0xffff82d08024ba90 to 0xffffffff81552790.
(XEN) [    3.593023] traps.c:2880:d0v0 Domain attempted WRMSR 00000000c0000083 from 0xffff82d0bffff020 to 0xffffffff815529d0.
(XEN) [    3.593026] traps.c:2880:d0v0 Domain attempted WRMSR 00000000c0000084 from 0x0000000000074700 to 0x0000000000047700.
(XEN) [    4.080747] traps.c:2880:d0v1 Domain attempted WRMSR 00000000c0000081 from 0xe023e00800000000 to 0x0023001000000000.
(XEN) [    4.080752] traps.c:2880:d0v1 Domain attempted WRMSR 00000000c0000082 from 0xffff82d0bfffe080 to 0xffffffff81551140.
(XEN) [    4.080755] traps.c:2880:d0v1 Domain attempted WRMSR 00000000c0000083 from 0xffff82d0bfffe0a0 to 0xffffffff81549340.
(XEN) [    4.080759] traps.c:2880:d0v1 Domain attempted WRMSR 0000000000000174 from 0x000000000000e008 to 0x0000000000000010.
(XEN) [    4.080762] traps.c:2880:d0v1 Domain attempted WRMSR 0000000000000175 from 0xffff8301392cffc0 to 0x0000000000000000.
(XEN) [    4.080765] traps.c:2880:d0v1 Domain attempted WRMSR 0000000000000176 from 0xffff82d08024ba90 to 0xffffffff81552790.
(XEN) [    4.080768] traps.c:2880:d0v1 Domain attempted WRMSR 00000000c0000083 from 0xffff82d0bfffe0a0 to 0xffffffff815529d0.
(XEN) [    4.080771] traps.c:2880:d0v1 Domain attempted WRMSR 00000000c0000084 from 0x0000000000074700 to 0x0000000000047700.
(XEN) [    4.085595] d0: Forcing write emulation on MFNs e0000-effff
(XEN) [    4.145925] Masked UR signaling on 0000:00:00.0
(XEN) [    4.145928] PCI add device 0000:00:00.0
(XEN) [    4.148416] PCI add device 0000:00:1a.0
(XEN) [    4.148854] PCI add device 0000:00:1c.0
(XEN) [    4.149238] PCI add device 0000:00:1c.4
(XEN) [    4.149614] PCI add device 0000:00:1c.5
(XEN) [    4.151966] PCI add device 0000:00:1d.0
(XEN) [    4.152254] PCI add device 0000:00:1e.0
(XEN) [    4.152551] PCI add device 0000:00:1f.0
(XEN) [    4.152987] PCI add device 0000:00:1f.2
(XEN) [    4.153201] PCI add device 0000:00:1f.3
(XEN) [    4.154495] PCI add device 0000:02:00.0
(XEN) [    4.966314] PCI add device 0000:03:00.0
(XEN) [    4.974440] PCI add device 0000:04:03.0
(XEN) [   15.916540] d0: Forcing read-only access to MFN fed00
