Settings for eth1:
	Supported ports: [ TP ]
	Supported link modes:   10baseT/Half 10baseT/Full 
	                        100baseT/Half 100baseT/Full 
	                        1000baseT/Half 1000baseT/Full 
	Supported pause frame use: No
	Supports auto-negotiation: Yes
	Advertised link modes:  10baseT/Half 10baseT/Full 
	                        100baseT/Half 100baseT/Full 
	                        1000baseT/Half 1000baseT/Full 
	Advertised pause frame use: Symmetric
	Advertised auto-negotiation: Yes
	Speed: Unknown!
	Duplex: Unknown! (255)
	Port: Twisted Pair
	PHYAD: 1
	Transceiver: internal
	Auto-negotiation: on
	MDI-X: Unknown
	Supports Wake-on: g
	Wake-on: d
	Current message level: 0x000000ff (255)
			       drv probe link timer ifdown ifup rx_err tx_err
	Link detected: no
